Value INTERFACE (\S+)
Value IP_ADDRESS (\S+)
Value STATUS (up|down|administratively down|deleted)
Value PROTO (up|down)

Start
  ^${INTERFACE}\s+${IP_ADDRESS}\s+\w+\s+\w+\s+${STATUS}\s+${PROTO} -> Record
  # Capture time-stamp if vty line has command time-stamping turned on
  ^Load\s+for\s+
  ^Time\s+source\s+is
