Value SYSTEM_ID ((\d+.\d+.\d+)|\S+)
Value TYPE (L\d)
Value INTERFACE (\S+)
Value IP_ADDRESS (\d+.\d+.\d+.\d+)
Value STATE (\S+)
Value HOLD_TIME (\d+)
Value CIRCUIT_ID (\S+)

Start
  ^${SYSTEM_ID}\s+${TYPE}\s+${INTERFACE}\s+${IP_ADDRESS}\s+${STATE}\s+${HOLD_TIME}\s+${CIRCUIT_ID} -> Record
  # Capture time-stamp if vty line has command time-stamping turned on
  ^Load\s+for\s+
  ^Time\s+source\s+is
