Value ADDRESS (\S+)
Value AGE (\d+|-)
Value MAC_ADDRESS (\S+|-)
Value TYPE (\S+)
Value INTERFACE (\S+)

Start
  ^IPv6\s+Address\s+Age\s+Link-layer\s+Addr\s+State\s+Interface\s*$$
  ^${ADDRESS}\s+${AGE}\s+${MAC_ADDRESS}\s+${TYPE}\s+${INTERFACE} -> Record
  # Capture time-stamp if vty line has command time-stamping turned on
  ^Load\s+for\s+
  ^Time\s+source\s+is
  ^\s*$$
  ^. -> Error
